; The NuFone Network's
; Open H.323 driver configuration
;
[general]
port = 1720
bindaddr = 0.0.0.0 
;tos=lowdelay
;
; You may specify a global default AMA flag for iaxtel calls.  It must be
; one of 'default', 'omit', 'billing', or 'documentation'.  These flags
; are used in the generation of call detail records.
;
;amaflags = default
;
; You may specify a default account for Call Detail Records in addition
; to specifying on a per-user basis
;
;accountcode=lss0101
;
; You can fine tune codecs here using "allow" and "disallow" clauses
; with specific codecs.  Use "all" to represent all formats.
;
disallow=all
;allow=all		; turns on all installed codecs
;disallow=g723.1	; Hm...  Proprietary, don't use it...
allow=gsm		; Always allow GSM, it's cool :)
;
; User-Input Mode (DTMF)
;
; valid entries are:   rfc2833, inband
; default is rfc2833
;dtmfmode=rfc2833
;
; Set the gatekeeper 
; DISCOVER			- Find the Gk address using multicast
; DISABLE			- Disable the use of a GK
; <IP address> or <Host name>	- The acutal IP address or hostname of your GK
;gatekeeper = DISABLE
;
;
; Tell Asterisk whether or not to accept Gatekeeper
; routed calls or not. Normally this should always
; be set to yes, unless you want to have finer control
; over which users are allowed access to Asterisk.
; Default: YES
;
;AllowGKRouted = yes
;
; Default context gets used in siutations where you are using 
; the GK routed model or no type=user was found. This gives you 
; the ability to either play an invalid message or to simply not 
; use user authentication at all.
;
;context=default
;
; H.323 Alias definitions
;
; Type 'h323' will register aliases to the endpoint
; and Gatekeeper, if there is one.
;
; Example: if someone calls time@your.asterisk.box.com
; Asterisk will send the call to the extension 'time' 
; in the context default
;
;   [default]
;   exten => time,1,Answer
;   exten => time,2,Playback,current-time
;
; Keyword's 'prefix' and 'e164' are only make sense when
; used with a gatekeeper. You can specify either a prefix 
; or E.164 this endpoint is responsible for terminating.
; 
; Example: The H.323 alias 'det-gw' will tell the gatekeeper
; to route any call with the prefix 1248 to this alias. Keyword
; e164 is used when you want to specifiy a full telephone
; number. So a call to the number 18102341212 would be 
; routed to the H.323 alias 'time'.
;
;[time]
;type=h323
;e164=18102341212
;context=default
;
;[det-gw]
;type=h323
;prefix=1248,1313
;context=detroit
;
;
; Inbound H.323 calls from BillyBob would land in the incoming
; context with a maximum of 4 concurrent incoming calls 
; 
;
; Note: If keyword 'incominglimit' are omitted Asterisk will not 
; enforce any maximum number of concurrent calls.
;
;[BillyBob]
;type=user
;host=192.168.1.1
;context=incoming
;incominglimit=4



